**Suomi National Polar-Orbiting Partnership (NPP) Visible Infrared Imaging Radiometer Suite (VIIRS) Aerosol Products Users Guide**

Version 2.0, April 2013

**1. Purpose of this Guide**

This VIIRS Aerosol Products Environmental Data Record (EDR) Users Guide is intended for users of the Aerosol and Suspended Matter EDRs generated from VIIRS. It provides a general introduction to the VIIRS instrument, data products, format, content, and their applications. It serves as an introduction and reference to more detailed technical documents about the VIIRS aerosol products and algorithms such as the Algorithm Theoretical Basis Document (ATBD) and Operational Algorithm Document (OAD) for the aerosol algorithms (see Section 9)

**2. Points of Contact**

For questions or comments regarding this document, please contact Istvan Laszlo ([Istvan.Laszlo@noaa.gov](mailto:Istvan.Laszlo@noaa.gov)) and/or Shobha Kondragunta (<Shobha.Kondragunta@noaa.gov>)

**3. Acronym List**

|  |  |
| --- | --- |
| AOD | Aerosol Optical Depth |
| AOT | Aerosol Optical Thickness |
| APSP | Aerosol Particle Size Parameter (Ångström Exponent) |
| AE | Ångström Exponent |
| ATBD | Algorithm Theoretical Basis Document |
| AVHRR | Advanced Very High Resolution Radiometer |
| CDFCB | Common Data Format Control Book |
| CLASS | Comprehensive Large Array-Data Stewardship System |
| EDR | Environmental Data Record |
| HDF5 | Hierarchical Data Format 5 |
| IDPS | Interface Data Processing System |
| IP | Intermediate Product |
| JPSS | Joint Polar Satellite System |
| LUT | Look Up Table |
| MODIS | Moderate Resolution Imaging Spectroradiometer |
| NCEP | National Center for Environmental Prediction |
| NPP | National Polar-orbiting Partnership |
| OAD | Operational Algorithm Description |
| QF | Quality Flag |
| RDR | Raw Data Records |
| SDR | Sensor Data Record |
| SM | Suspended Matter |
| TOA | Top of Atmosphere |
| VCM | VIIRS Cloud Mask |
| VIIRS | Visible Infrared Imaging Radiometer Suite |

Table 1: Acronyms

**4. Document Definitions**

This document will refer to aerosol optical thickness (AOT) instead of aerosol optical depth (AOD) for consistency with other VIIRS Aerosol Product documentation.

Aerosol particle size parameter (APSP) is defined as the Ångström Exponent (α) (see ATBD for more details).

**5. VIIRS**

**5.1 Overview**

VIIRS is one of the five instruments on board the Suomi NPP satellite. It is a scanning radiometer with capabilities that are intended to extend and improve upon the heritage of AVHRR and MODIS. VIIRS data is used to measure cloud and aerosol properties, ocean color, sea and land surface temperature, ice motion and temperature, fires, and Earth’s albedo. The NPP satellite, and therefore VIIRS, has an 824 km sun-synchronous orbit (i=98.7º) with a 1:30pm an equator crossing time at the ascending node. It achieves global coverage every day and has a repeat cycle of approximately 16 days. VIIRS has a swath width of 3040 km with a spatial resolution of ~375 m at nadir in the Imagery (I) Bands and ~750 m at nadir in the Moderate (M) Bands. Through a system of pixel aggregation techniques, VIIRS controls pixel growth towards the edge of scan such that the pixel sizes are comparable to nadir. For more information about this “bow-tie removal” aggregation scheme, look at the SDR User’s Guide (<https://cs.star.nesdis.noaa.gov/NCC/UsersGuideVIIRS>, beginning on page 29) and the Imagery Products ATBD (<http://npp.gsfc.nasa.gov/science/sciencedocuments/ATBD_122011/474-00031_Rev-Baseline.pdf>, beginning on page 26) Additional information and specifications for NPP and VIIRS can be found at <http://npp.gsfc.nasa.gov/spacecraft_inst.html>.

**5.2 Data Processing Chain**

The NPP satellite transmits raw instrument data to the Command, Control, and Communications Segment (C3S) which is then routed to the Interface Data Processing Segment (IDPS). The IDPS processes the Raw Data Records (RDRs) to create Sensor Data Records (SDRs), which are subsequently processed into Environmental Data Records (EDRs). The IDPS then transmits RDRs, SDRs, and EDRs to CLASS for distribution and archiving.

**5.3 Data Records Overview**

VIIRS data products are stored and distributed in HDF5 format. There is no special “HDF-NPP” library for use with these data files, but the NPP data products were designed using the native HDF5 library. VIIRS files from IDPS contain a single granule of a single data type. Granules are associated with an integer number of sensor scans, so the definition varies between sensors and data products. VIIRS aerosol product granules are 48 scan lines, or approximately 86 seconds in length, and the pixel-level M-band resolution data is contained in 768 x 3200 arrays. The CDFCBs provide information on other products and their granule lengths (see Section 9). Due to the relatively short granule length and the data resolution, users should expect approximately 1000 files (sizes are ~1.3 MB each for aggregated aerosol EDR and geolocation, ~15 MB for pixel level Intermediate Product (IP) AOT, 1.5 MB for pixel level Suspended Matter, and ~78 MB each for M-band pixel-level geolocation) per data product per day. Some data sources downstream of IDPS may post-process data, including aggregating multiple granules or packaging different data types into a single file which will alter these approximations (see Section 5.4).

**5.3.1 Raw Data Records (RDRs)**

NPP RDRs are binary data generated by the sensors on board the NPP spacecraft. They contain engineering and house-keeping data for spacecraft and sensor monitoring as well as science data for the production for SDRs. The required inputs for generating SDR products are verified RDRs, which contain the information that is converted into calibrated TOA radiance, reflectance, and brightness temperature, along with other sensor calibration information. A comprehensive discussion of the contents and structure of RDR products is available in Volume II of the CDFCB (see Section 9)

**5.3.2 Sensor Data Records (SDRs)/Level 1B**

NPP SDRs contain calibrated and geolocated TOA radiance and reflectance data produced from processing the RDRs along with quality flags and metadata. An excellent overview of the SDR products is available in the SDR User’s Guide at <https://cs.star.nesdis.noaa.gov/NCC/UsersGuideVIIRS> and a complete description is available in Volume III of the CDFCB (see Section 9)

**5.3.3 Environmental Data Records (EDRs)/Level 2**

NPP EDRs contain derived biogeophysical parameters that are broadly categorized into four sections: land, ocean, imagery and clouds, and aerosols. Only the aerosol product EDRs are discussed in this document (see Section 7), but a full list of all available EDRs is located at <http://npp.gsfc.nasa.gov/science/DataProducts.html> and described in more detail in Volume IV, Parts II-IV of the CDFCB (see Section 9)

**5.3.4 Intermediate Products (IPs)**

Intermediate products are the retrieval byproducts or data subsets that are created through processing that are required for a later primary data product’s generation or used as input for secondary processing. Some IPs such as the cloud mask and aerosol optical thickness are delivered and available to the user. The contents of IP AOT files are discussed in more detail in Section x of this document.

**5.3.5 Geolocation**

Unless packaged through post processing, VIIRS Geolocation data is stored in separate geolocation files that must be used in conjunction with SDRs, EDRs, and IPs. The contents of the geolocation files related to the aerosol products are discussed in more detail in Section 7 of this document and a full description of all geolocation files can be found in Volume IV, Part I of the CDFCB (see Section 9).

**5.4 Data Availability**

**5.4.1 CLASS**

The primary data source for NPP products is through NOAA’s CLASS web interface ([www.class.noaa.gov](http://www.class.noaa.gov); Note that there are actually three CLASS sites that users are directed to from this link depending on usage and maintenance of each site. Be careful bookmarking one of the specific sites as it may be temporarily down when it is accessed explicitly). All aerosol products described in this document are available from this source. Data delivered to CLASS from the IDPS has a latency specification of 6 hours from observation, but can increase due to data issues along the processing chain described in Section 5.2. On CLASS, users will have options with respect to the format in which they prefer data. Data searches on CLASS can be defined by data type, date and time range, geolocation, node, granule ID, and beginning orbit number. When ordering data, it is possible to request a certain level of packaging and aggregation of the NPP data files. By default, CLASS will package and aggregate data orders, meaning they will package corresponding geolocation files together with the requested data files and aggregate four 86-second granules into a single file. This can be changed on a case-by-case basis on the order form or can be re-set in the user preferences to apply to all orders. There are two basic ways to order data from CLASS: ad hoc orders and subscriptions. Within the ad hoc category, there are three options. If the user elects to search using the normal “Search” button, file orders will be restricted to 100 files. This option is useful if you would like to view and inventory listing of the data available within your search parameters and select a small number of specific files. If the user is confident about their search parameters, they may also use the “Quick Search and Order” button that will skip the inventory list and allow users to order up to 1000 files each time. For larger order sizes, users can request Block Orders through the CLASS helpdesk (class.help@noaa.gov). This access will allow orders of up to 3000 files. Finally, subscriptions are also available to users who require regular data access in the form of an automatic push or pull distribution. Requests for subscriptions must be sent to the CLASS helpdesk. Ad hoc data orders are delivered using FTP, where data will remain for 48 hours (requests can be made for longer holding times). An excellent visual walk through of the NPP data order procedure is available at: http://www.class.ngdc.noaa.gov/notification/pdfs/CLASS\_Tutorial\_NPPDataAccess\_20110909.pdf. What about recent changes where you can order 90 days worth of data and a tar file is created?

**5.5 Filenames**




Figure 1: NPP Filename Fields with AOT EDR Filename Example

Figure 1 describes the file naming convention of NPP data products. A full description of each of the file name data field along with applicable values is available in the CDFCB, Volume 1 beginning on page 22. The relevant Data Product IDs for the aerosol products are IVAOT (Aerosol IP), VAOOO (Aerosol EDR), VSUMO (Suspended Matter EDR), GAERO (Aerosol EDR Geolocation), and GMTCO (Pixel-Level Terrain Corrected Geolocation). It is worth noting that the NPP granule ID does not appear in the file name. The granule ID is available within each data file as the metadata item “N\_Granule\_ID”. It is written as a 15 character string, where the first three characters are the satellite identifier of NPP and the next 12 numeric characters specify the number of tenths of a second since the first ascending node after launch.

**6. VIIRS Aerosol Algorithm**

**6.1 VIIRS Bands Relevant to the Aerosol Products**

VIIRS has 22 spectral bands, of which 16 are M-bands (~750 m resolution at nadir) and 5 are I-bands (~375 m m resolution at nadir). Table 2 is a chart of the bands used when creating the aerosol products.

|  |  |  |  |
| --- | --- | --- | --- |
| Band Name | Wavelength(µm) | Bandwidth | Aerosol Algorithm Use |
| M1 | 0.412 | 0.0200 | Land Retrieval |
| M2 | 0.445 | 0.0180 | Land Retrieval, Land Angstrom Exponent |
| M3 | 0.488 | 0.0200 | Land Retrieval, Internal Tests |
| M4 | 0.555 | 0.0200 | Internal Tests |
| M5 | 0.672 | 0.0200 | Land Retrieval (Reference), Ocean Retrieval, Internal Tests, Land Angstrom Exponent |
| M6 | 0.746 | 0.0150 | Ocean Retrieval |
| M7 | 0.865 | 0.0390 | Ocean Retrieval (Reference), Internal Tests, Ocean Angstrom Exponent |
| M8 | 1.240 | 0.0200 | Ocean Retrieval, Internal Tests |
| M9 | 1.378 | 0.0150 | Internal Tests |
| M10 | 1.610 | 0.0600 | Ocean Retrieval, Internal Tests, Ocean Angstrom Exponent |
| M11 | 2.250 | 0.0500 | Land Retrieval, Ocean Retrieval, Internal Tests |
| M12 | 3.700 | 0.1800 | Internal Tests |
| M15 | 10.7625 | 1.0000 | Internal Tests |
| M16 | 12.0125 | 0.9500 | Internal Tests |

Table 2: VIIRS Aerosol Bands

A comprehensive chart of the VIIRS bands can be found at <http://www.star.nesdis.noaa.gov/jpss/documents/meetings/2011/NPP_Users_Workshop/02.0%20NPP%20SDR%20Overview-July%2023%202011%20Weng.pdf> on slide 17.

**6.2 Summary of the Aerosol Algorithm**

The VIIRS Aerosol Algorithm retrieves AOT at a pixel level for a range of 11wavelengths (0.412, 0.445, 0.488, 0.550, 0.555, 0.672, 0.746, 0.865, 1.240, 1.610, and 2.250 microns). The current version of the algorithm does not retrieve aerosol properties over bright surfaces, in cloud-affected pixels, over inland water such as the Great Lakes, or at night. The AOT is calculated separately for land and ocean using a LUT of pre-computed values for several atmospheric parameters to simplify radiative transfer calculations. Pixel level AE is then calculated from AOT at two different wavelengths (0.455 and 0.672 microns over land and 0.865 and 1.610 microns over ocean). The pixel level AOT and AE products are aggregated to create the EDR (see Section 6.3). The suspended matter type for each pixel is derived for pixels with an AOT greater than a specified threshold. Possible suspended matter types and the conditions under which they are chosen are shown in Table 3. In depth descriptions of the algorithms are available in the Aerosol Optical Thickness and Particle Size Parameter ATBD and the Suspended Matter ATBD, and algorithm flow and logic charts are provided in Figures 1, 2, 3, 4, and 5 of the Aerosol Products OAD (see Section 9).

|  |  |  |
| --- | --- | --- |
| **SM Type** | **Conditions over Land** | **Conditions over Ocean** |
| **Ash** | VIIRS Cloud Mask identifies the presence of volcanic ash (tuned out in IDPS build as of November 2, 2012 due to false positives) | |
| **Dust** | AOT at 550 nm > 0.15 and dust Land Aerosol Model selected (See EDR Quality Flags in Appendix A) | AOT at 550 nm > 0.15 and fine mode fraction < 0.2 |
| **Smoke** | AOT at 550 nm > 0.15 and non-dust Land Aerosol Model selected (high/low absorbing smoke; clean/polluted urban aerosol) (See EDR Quality Flags in Appendix A) | AOT at 550 nm > 0.15, fine mode fraction ≥ 0.5 (See EDR Quality Flags in Appendix A) |
| **Sea Salt** | N/A | 0.15 < AOT at 550 nm < 0.3 and 0.2 ≤ fine mode fraction < 0.5 |
| **Unknown (Undetermined SM Type)** | N/A | AOT at 550nm ≥ 0.3 and 0.2 ≤ fine mode fraction < 0.5 (See EDR Quality Flags in Appendix A) |
| **None (No SM)** | AOT at 550 nm ≤ 0.15 | |

Table 3: Suspended Matter Types and Conditions Under Which Each Type is Chosen

**6.3 Aggregation of the Aerosol EDR from the Aerosol IP**

The aerosol EDR is created from the IP product through a system of quality checks, filtering, and spatial aggregation of 8x8 pixel IP values. The logic flow for creating each 8x8 pixel horizontal cell within the aerosol EDR is shown in Figure 2 below. The top two pixel-level quality flags referenced in Figure 2 are “high” and “degraded”. The conditions for each of these quality flags are described in Table 4, along with the conditions for “excluded” quality pixels (have a retrieval but are excluded from the aggregation process), and “not produced” quality pixels (no retrieval). The EDR quality flags referenced in Figure 2 are discussed in more detail in Appendix A. The corresponding aerosol EDR geolocation is determined by simply taking the central geolocation point for each horizontal cell.

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
|  | **Not Produced** | **Excluded** | **Degraded** | **High** |
| **AOT** | Solar zenith angle > 80o, Missing or saturated channel reflectance (L: M1, M2, M3, M5, M8, M11; O: M5, M6, M7, M8, M10, M11), Missing ancillary data (wind speed, wind direction, precipitable water, surface air temperature, column ozone, surface pressure, surface height), Probably or confidently cloudy, Snow/ice present, Fire present, Inland or coastal water, Sun glint present, Turbid water present, Bright surface present | Retrieved AOT at 550nm is out of spec range (0.0-2.0), Missing channel reflectance/brightness temperature (L: M3, M5, M7, M8, M9, M10, M11, M12, M15, M16; O: M3, M4, M15, M16) | 65o ≤ Solar Zenith Angle < 80o, Cloud shadow present, Cirrus present, Adjacent pixel probably or confidently cloudy, Volcanic ash present, Soil dominant pixel, Retrieval residual beyond threshold | Otherwise |
| **APSP** | Non-positive AOT at the channels used for AE Calculation (L: M2/M5; O: M7/M10) | Out of spec range (-1.0-3.0) | AOT at 550 nm < 0.15 | Otherwise |

Table 4: Pixel-level quality flag conditions for AOT and APSP



Figure 2: IP to EDR Aggregation

**7. VIIRS Aerosol Products**

The VIIRS aerosol algorithm produces several data products that are available to users via CLASS. The following sections describe the data that appears in unaggregated, unpackaged granules of the aerosol data products. Helpful tools for working with these data products are described in Appendix B.

**7.1 IP AOT**

The VIIRS aerosol IP contains AOT at 550 nm (see Section 6.2), slant column AOT at 550 nm, and Angstrom Exponent. This is a pixel level (~750 m) retrieval that is stored in 768 X 3200 floating point array.There are numerous quality flags (described in detail in Appendix A) which are in 8-bit integer format. Finally, the HDF5 file contains all the metadata for the granule. To match an Aerosol IP to its corresponding Aerosol Geolocation file, ensure that the date, start time, end time, and orbit number in each filename are identical. For example,

|  |
| --- |
|  |

**GMTCO\_npp\_d20120104\_t0001202\_e0002443\_b00959\_c201204022745955416\_noaa\_ops.h5**

is the corresponding geolocation file for the Aerosol IP

**IVAOT\_npp\_d20120104\_t0001202\_e0002443\_b00959\_c201204022745955416\_noaa\_ops.h5**


****

Figure 3: IP AOT file opened in HDFView to examine details of data structures and metadata

One notable difference between Aerosol IP and Aerosol EDR (Section 7.2) is that the IP AOT file contains information from Navy Aerosol Analysis and Prediction System (NAAPS). When there are pixels with no retrievals due to clouds or bright surface or night time, NAAPS predicted AOT interpolated to VIIRS observation time are used to fill in. If NAAPS predictions are not available, a climatology is used. This information is for downstream use by the land surface albedo retrievals and not used by the Aerosol EDR. The NAAPS values in the Aerosol IP file are explicitly flagged and should not be used when VIIRS Aerosol IP data are analyzed. The quality flags for Aerosol IP are 0 for good, 1 for degraded, 2 for excluded, and 3 for not produced. It is recommended that only data with quality flag 0 be used.

**7.2 Aerosol EDR**

The VIIRS aerosol EDR contains the AOT for 11 wavelengths ranging from 0.412-2.25 microns (see Section 6.2) and the Angstrom Exponent. These values are stored as a 96 x 400 array of 16-bit integers with the corresponding scale and offset stored separately in the granule. To convert the 16-bit integers to floating point numbers, users need to multiply by the scale first, and then add the offset. There are numerous quality flags (described in detail in Appendix B) which are in 8-bit integer format. The small mode fraction is provided in 8 bit integer format. Finally, the HDF5 file will contain all the metadata for the granule. All the data in this file is at the horizontal cell resolution (8x8 pixels, approximately 6km at nadir). The Aerosol EDR requires a corresponding Aerosol EDR geolocation for analysis. To match an Aerosol EDR to its corresponding Aerosol Geolocation file, ensure that the date, start time, end time, and orbit number in each filename are identical. For example, is the corresponding geolocation file for the Aerosol EDR

Figure 4: Aerosol EDR File opened in HDFView to examine details of data structures and metadata

**7.3 Aerosol EDR Geolocation**

The aerosol EDR geolocation file contains the geolocation information, overpass time and satellite geometry at the horizontal cell resolution to be used in conjunction with the AOT and APSP data in the Aerosol EDR files. Note that the start and mid times are expressed in milliseconds after the launch basetime (1698019234000000).

Figure 5: Aerosol Geolocation File opened in HDFView to examine details of data structures and metadata

**7.4 Suspended Matter EDR**

The Suspended Matter EDR contains the suspended matter type (see Table 3) in 8-bit integer format and the smoke concentration in 16-bit integer format with the corresponding scale and offset for floating point conversion. All data in this file is at the pixel resolution (~750 m at nadir). There are also numerous 8-bit integer quality flags (described in more detail in Appendix A and also in the Aerosol Product OAD). The Suspended Matter EDR requires a corresponding terrain-corrected M-Band pixel-level geolocation for analysis. To match a Suspended Matter EDR to its corresponding geolocation file, ensure that the date, start time, end time, and orbit number in each filename are identical. For example, is the corresponding geolocation file to the Suspended Matter EDR file

Figure 6 Suspended Matter EDR File opened in HDFView to examine details of data structures and metadata

**7.5 M-Band Terrain-Corrected Geolocation**

Although it is not an output product of the aerosol algorithm, the M-Band pixel-level terrain-corrected geolocation product is required for use with the Suspended Matter EDR products. The file contains geolocation information, overpass time and satellite geometry at the M-Band pixel resolution (~750 m at nadir). Note that the start and mid times are expressed in milliseconds after the launch basetime (1698019234000000).

Figure 7: M-Band Terrain-Corrected Geolocation File opened in HDFView to examine details of data structures and metadata

**8. Known Issues to Date**

The VIIRS Aerosol team has identified the following data quality problems that the user should be aware of:

* Artificially high AOT and APSP in the snow melt region of the Northern Hemisphere during the Spring thaw
* Low AOT bias over ocean in dust outflow regions
* Proportion of AOT attributed to small particles is too high over ocean
* Currently, there is no skill in systematically retrieving APSP information over land
* Overabundance of smoke, and not enough dust in Suspended Matter product
* Overabundance of ephemeral water over bright surfaces (though no retrieval in either case)
* Some internal tests (for detection of snow/ice, bright pixel, fire detection, etc.) are under evaluation for updates
* There are no retrievals (by design) over inland water bodies
* In heavy aerosol regions (dust and smoke plumes), the pixel-level AOT is often out of range (0.0 – 2.0) and is therefore excluded from aggregation and the EDR product
* An inadvertent error introduced in the operational aerosol code resulted in significantly degraded aerosol EDRs for the following timeframe, invalidating the aerosol beta maturity results for the period: 10/15/2012 to 11/27/2012. Users should be aware that within this timeframe, AOT values were retrieved for confidently cloud areas (as determined by the VIIRS cloud mask) where there should not have been retrievals, leading to increased AOT values and significantly degraded products.

The VIIRS Aerosol team strongly recommends that the following quality flags be applied:

* Use only products that are flagged as High (QF = 3) or Medium (QF = 2) quality for Aerosol EDR and High (QF=0) for Aerosol IP.

**9. Additional Documentation**

**9.1 Common Data Format Control Book (CDFCB)**

The CDFCB documents provide in depth technical information about the NPP data products. They are available publically at <http://npp.gsfc.nasa.gov/science/documents.html>. A summary of the contents are below.

|  |  |
| --- | --- |
| Volume I | Overview |
| Volume II | RDR Formats |
| Volume III | SDR/TDR Formats |
| Volume IV | EDR/IP/ARP and Geolocation Formats |
| Volume V | Metadata |
| Volume VI | Ancillary Data, Auxiliary Data, Messages and Reports |
| Volume VII | Downlink Formats (Application Packets) |
| Volume VIII | LUT Formats |

The CDFCB sections relevant to the Aerosol Products are Volume I and Volume IV, Parts I and II.

**9.2 Algorithm Theoretical Basis Document (ATBD)**

The AOT/APSP and Suspended Matter ATBDs provide a description of the physical theory and mathematical background of the aerosol algorithm as well as implementation details and describes the assumptions and limitations of the scientific approach. It also identifies the VIIRS and non-VIIRS sources for required input data. The ATBD is available publically at <http://npp.gsfc.nasa.gov/science/documents.html>.

**9.3 Operational Algorithm Description (OAD)**

The Aerosol Products OAD provides a description of the aerosol algorithm and end-user data products in computer science terms. It is available publically at <http://npp.gsfc.nasa.gov/science/documents.html>

**Appendix A: VIIRS Aerosol IP Quality Flags**

**A.1. IP Quality Flags**

**A.1.1. QF1**

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| Flag | Values | Bits | Conditions | Notes |
| AOT Quality | 00 = 0 =High 01 = 1 = Degraded 10 = 2 = Excluded 11 = 3 = Not Produced | 2 | AOTNOTPRODUCED(3):   * Solar zenith angle > 80° * Missing channel reflectance * Over land: M1, M2, M3, M5, M8, M11 * Over water: M5, M6, M7, M8, M10, M11 * Missing ancillary model data * Wind speed, wind direction, precipitable water, surface air temperature, column ozone, surface pressure, surface height * Probably or confident cloudy * Snow/ice present * Fire present * Unfavorable surface: inland water or coastal * Internal test * Over land: sun glint; fire; snow/ice * Over water: sun glint; turbid water; snow/ice * Bright surface over land * Bright pixel index ()<0.05 and Reflectance at M11 > 0.3   AOTEXCLUDED(2):   * Use tertiary ancillary model data (obsolete) * Retrieved AOT550 out of spec range [0,2] * Internal test * Missing channel reflectance or brightness temperature (M3,M5,M7,M8,M9,M10,M11,M12, M15, M16 over land; M3,M4,M15,M16 over water)   AOTDEGRADED(1):   * 65° ≤ Solar zenith angle < 80° * Use secondary ancillary model data (obsolete) * Presence of cloud shadow ; cirrus ; adjacent pixel cloud confidence level being probably or confidently cloudy ; volcanic ash * Soil dominant over land (bright pixel index ≤ 0.2) * Retrieval residual beyond the threshold * Minimum residual > 0.05 when AOT550 > 0.5 over land * Minimum residual > 0.5 when AOT550 > 0.5 over water   AOTHIGH(0): otherwise |  |
| Ångström exponent Quality | 00 = 0 = High 01 = 1 = Degraded 10 = 2 = Excluded 11 = 3 = Not Produced | 2 | Set to be same as the Aerosol optical thickness quality  AOTNOTPRODUCED(3):   * Nonpositive AOT at channels used for AE calculation (M2 / M5 over land; M7 / M10 over water)   AOTEXCLUDED(2):   * Out of spec range [-1.0, 3.0]   AOTDEGRADED(1):   * Low AOT 550 (< 0.15)   AOTHIGH(0): otherwise |  |
| Suspended Matter Type Quality | 00 = 0 = High 01 = 1 = Degraded 10 = 2 = Excluded 11 = 3 = Not Produced | 2 | Set to be same as AOT quality flag  AOTNOTPRODUCED(3);  AOTEXCLUDED(2);   * 0.15 < AOT550 < 0.5   AOTDEGRADED(1);  AOTHIGH(0):  if volcanic ash is detected , the SM type quality is set to be HIGH no matter what the quality flag for AOT is. |  |
| Cloud Mask Quality | 00 = 0 = Poor 01 = 1 = Low 10 = 2 = Medium 11 = 3 = High | 2 | Direct copy from VIIRS cloud mask (VCM) without modification |  |

**A1.2. QF2**

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| Flag | Values | Bits | Conditions | Notes |
| Cloud Detection Result & Confidence Indicator | 00 = 0 = Confident Clear 01 = 1 = Probably Clear  10 = 2 = Probably Cloudy  11 = 3 = Confident Cloudy | 2 | Direct copy from VCM, with one modification on confident clear case  CM\_CONF\_CLOUDY (3)  CM\_PROB\_CLOUDY(2)  CM\_PROB\_CLEAR(1)  CM\_CONF\_CLEAR(0):  if the heavy aerosol flag is turned on in VCM |  |
| Adjacent Pixel Cloud Confidence Value | 00 = 0 = Confident Clear 01 = 1 = Probably Clear  10 = 2 = Probably Cloudy  11 = 3 = Confident Cloudy | 2 | Initially copied from VCM, but subsequently modified to be the most cloudy category available from the adjacent 3x3 pixel cloud confidence flags  CM\_CONF\_CLOUDY (3)  CM\_PROB\_CLOUDY(2)  CM\_PROB\_CLEAR(1)  CM\_CONF\_CLEAR(0) |  |
| Land/Water Background | 000 = 0 = Land & Desert 001 = 1 = Land, No Desert  010 = 2 = Inland Water 011 = 3 = Sea Water  101 = 5 = Coastal  110 = 6 = Ephemeral Water | 3 | Direct copy from VCM, add a new surface type if ephemeral water is detected in the internal test over land.  CM\_DESERT (0)  CM\_LAND (1)  CM\_IN\_WATER(2)  CM\_SEA\_WATER (3)  CM\_COASTAL (5)  AOT\_EPHWAT (6):   * New type added through internal test over land |  |
| Bad SDR | 1 = Yes 0 = No | 1 | AOTQFYES(1):   * If channel reflectance or brightness temperature are missing (<-999.0)   Over land: M1-M12,M15,M16  Over water: M3- 11, M15,M16  AOTQFNO(0): otherwise |  |

**A.1.3. QF3**

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| Flag | Values | Bits | Conditions | Notes |
| Day/Night Flag | 00 = 0 =Day 01 = 1 =Low Sun, Degraded  10 = 2 = Twilight, Excluded  11 = 3 = Night | 2 | AOTNIGHT (3):   * Solar zenith angle > 85°   AOTSOLZAEX (2):   * 80° < Solar zenith angle ≤ 85°   AOTSOLZADEG (1):   * 65° < Solar zenith angle ≤ 80°   AOTDAY (0):  Solar zenith angle ≤ 65° |  |
| Interpolation / NAAPS / Climatology Processing Used | 000 = 0 = None 001 = 1 = Interpolation only  010 = 2 = Interpolation & Climatology/NAAPS  011 = 3 = Climatology/NAAPS | 3 | AOTCLIMO (3):   * If there is no good or degraded quality retrieval available within the searching window (41x41 pixels) * Use NAAPS (if available) or climatology AOT550 only; aerosol model information is from climatology   AOTINTCLIMO (2):   * Ratio of the total weight of pixels with available retrievals to the total weight of all pixels within the searching window < 0.25 * Combine interpolated (weighted average of good/degraded retrievals) and NAAPS/climatology AOT550; aerosol model information is from the retrieval with highest weight (if available) or climatology.   AOTINT (1):   * Above weight ratio ≥ 0.25 * Use interpolated (weighted average of good/degraded retrievals) AOT550 only; aerosol model information is from the retrieval with highest weight (if available) or climatology.   AOTNOINTCLIMO (0):   * Good/degraded aerosol retrieval is available |  |
| Sun Glint | 000 = 0 = None 001 = 1 = Geometry Based  010 = 2 = Wind Speed Based 011 = 3 = Geometry & Wind  100 = 4 = Internal  101 = 5 = Internal & Geometry  110 = 6 = Internal & Wind  111 = 7 = All | 3 | Over land: determined by internal test  over water: initially copied from VCM and internal test also checks |  |

**A.1.4. QF4**

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| Flag | Values | Bits | Conditions | Notes |
| Snow/Ice | 1 = Yes  0 = No | 1 | Initially copied from VCM, internal tests also check for snow/ice  AOTQFYES (1):   * VCM identified or internal tests detected   AOTQFNO(0): |  |
| Cirrus | 1 = Yes  0 = No | 1 | Initially copied from VCM, internal tests also check for cirrus over land  CM\_CLOUD (1):   * VCM identified or internal test (over land) detected   CM\_NO\_CLOUD (0) |  |
| Cloud Shadow | 1 = Yes  0 = No | 1 | Copied from VCM |  |
| Fire | 1 = Yes  0 = No | 1 | Initially copied from VCM, internal tests also check fire over land  CM\_FIRE (1)   * VCM identified or internal test (over land) detected   CM\_NO\_FIRE (0) |  |
| Bright Pixel | 00 = 0 = Dark  01 = 1 = Soil Dominated  10 = 2 = Bright | 2 | Land only  AOTBRIGHT (2):   * Bright pixel index ()<0.05 and Reflectance at M11 > 0.3   AOTSOIL (1):   * Bright pixel index ≤ 0.2, soil dominated.   AOTVEG (0):   * Initial value. |  |
| Turbid/Shallow Water | 1 = Yes  0 = No | 1 | AOTQFYES (1):   * Detected by internal test over water   AOTQFNO (0) |  |
| Ash | 1 = Yes  0 = No | 1 | Copied from VCM  AOTQFYES (1)  AOTQFNO (0) |  |

**A.1.5. QF5**

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| Flag | Values | Bits | Conditions | Notes |
| Low AOT – SM Typing Excluded | 1 = Yes  0 = No | 1 | AOTQFYES (1):   * If 0.15 < AOT550 < 1.0   AOTQFNO (0):   * AOT550 ≤ 0.15 – no suspended matter * AOT550 ≥ 1.0 |  |
| Low AOT – SM Detection Excluded | 1 = Yes  0 = No | 1 | AOTQFYES (1):   * If 0.15 < AOT550 < 0.5   AOTQFNO (0):   * AOT550 ≤ 0.15 – no suspended matter * AOT550 ≥ 0.5 |  |
| AOT Out of Spec Range | 1 = Yes  0 = No | 1 | AOTQFYES (1):   * If AOT550 < 0.0 or AOT550 > 2.0   AOTQFNO (0) |  |
| APSP Out of Spec Range | 1 = Yes  0 = No | 1 | AOTQFYES (1):   * If AE < -1.0 or AE > 3.0   AOTQFNO (0) |  |
| Low AOT, APSP Excluded | 1 = Yes  0 = No | 1 | AOTQFYES (1):   * If AOT550 < 0.15   AOTQFNO (0) |  |
| Residual Threshold Exceeded | 1 = Yes  0 = No | 1 | AOTQFYES (1):   * Minimum residual > 0.05 when AOT550 > 0.5 over land * Minimum residual > 0.5 when AOT550 > 0.5 over water   AOTQFNO (0) |  |

**A.2. EDR Quality Flags**

**A.2..1. QF1**

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| Flag | Values | Bits | Conditions | Notes |
| AOT Quality | 11 = 3 = High 10 = 2 = Medium 01 = 1 =Low 00 = 0 = Not Produced | 2 | **High:** Number of good quality pixel AOT retrievals > 16 (1/4 the total number of pixels in aggregated horizontal cell) **Medium:** Number of good quality retrievals ≤ 16 and the number of good/degraded quality retrievals ≥ 16 **Low:** Number of good/degraded quality retrievals < 16 **Not Produced:** No good/degraded quality retrievals, neither land or sea water dominant (number of land or ocean pixels < half the number of good/degraded pixels in the horizontal cell), ellipsoid fill in the geolocation, night scan, has a pixel with a solar zenith angle between 80º and 85º but no pixel with a solar zenith angle between 65º and 80º |  |
| APSP Quality | 11 = 3 = High 10 = 2 = Medium 01 = 1 =Low 00 = 0 = Not Produced | 2 | **High:** Number of good quality pixel APSP retrievals > 16 (1/4 the total number of pixels in aggregated horizontal cell) **Medium:** Number of good quality retrievals ≤ 16 and the number of good/degraded quality retrievals ≥ 16 **Low:** Number of good/degraded quality retrievals < 16 **Not Produced:** No good/degraded quality retrievals, neither land or sea water dominant (number of land or ocean pixels < half the number of good/degraded pixels in the horizontal cell), ellipsoid fill in the geolocation, night scan |  |
| Land, Ocean, or Not Produced | 00 = 0 = Land 01 = 1 = Ocean 10 = 2 = Not Produced | 2 | **Land:** Number of land/desert pixels ≥ half the total good/degraded pixels within the horizontal cell **Ocean:** Number of sea water pixels > half the total good/degraded pixels within the horizontal cell |  |
| AOT out of Spec Range | 1 = Yes 0 = No | 1 | **Yes:** AOT at 550 nm of any pixel in the 8x8 horizontal cell is out of spec range (0.0-2.0) |  |
| APSP out of Spec Range | 1 = Yes 0 = No | 1 | **Yes:** APSP of any pixel in the 8x8 horizontal cell is out of spec range (-1.0-3.0) |  |

**A.2.2. QF2**

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| Flag | Values | Bits | Conditions | Notes |
| Cloud Contamination | 1 = Yes 0 = No | 1 | **Yes:** Any pixel in the 8x8 horizontal cell is not confidently clear |  |
| Cloud adjacent to cell | 1 = Yes 0 = No | 1 | **Yes:** Any pixel in the 8x8 horizontal cell has their cloud adjacency flagged as probably or confidently cloudy |  |
| Cirrus Contamination | 1 = Yes 0 = No | 1 | **Yes:** Any pixel in the 8x8 horizontal cell has cirrus |  |
| Bad SDR | 1 = Yes 0 = No | 1 | **Yes:** Any pixel in the 8x8 horizontal cell has bad SDR |  |
| Sunglint | 1 = Yes 0 = No | 1 | **Yes:** Any pixel in the 8x8 horizontal cell has sunglint |  |
| Cloud Shadow | 1 = Yes 0 = No | 1 | **Yes:** Any pixel in the 8x8 horizontal cell has cloud shadow |  |
| Snow/Ice | 1 = Yes 0 = No | 1 | **Yes:** Any pixel in the 8x8 horizontal cell has snow/ice |  |
| Fire | 1 = Yes 0 = No | 1 | **Yes:** Any pixel in the 8x8 horizontal cell has fire |  |

**A.2.3. QF3**

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| Flag | Values | Bits | Conditions | Notes |
| Low sun, degraded | 1 = Yes 0 = No | 1 | **Yes:** Any pixel in the 8x8 horizontal cell has the day/night flag set to 'Low sun, degraded' (65º < Solar zenith angle ≤ 80º) |  |
| Low sun, excluded | 1 = Yes 0 = No | 1 | **Yes:** Any pixel in the 8x8 horizontal cell has the day/night flag set to 'Low sun, excluded' (80º < Solar zenith angle ≤ 85º) |  |
| Bright surface (land)/Shallow or Turbid Water (ocean) | 1 = Yes 0 = No | 1 | **Yes:** Any pixel in the 8x8 horizontal cell has a bright pixel (land) or turbid/shallow water (ocean) |  |
| Low AOT, APSP Excluded | 1 = Yes 0 = No | 1 | **Yes:** Any pixel in the 8x8 horizontal cell has excluded APSP |  |

**A.2.4. QF4**

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| Flag | Values | Bits | Conditions | Notes |
| Land Model Aerosol Index (land) | 100 = 4 = Urban, Polluted 011 = 3 = Urban, Clean 010 = 2 = Smoke, Low Absorption 001 = 1 = Smoke, High Absorption 000 = 0 = Dust | 3 |  | Selects the dominant aerosol model (largest number of pixels involved in the EDR aggregation) over land; See AOT ATBD for all model details |

**A.2.5. QF5**

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| Flag | Values | Bits | Conditions | Notes |
| Small Mode Aerosol Model (ocean) | 011 = 3 = Fine mode 4 010 = 2 = Fine mode 3 001 = 1 = Fine mode 2 000 = 0 = Fine mode 1 111 = 7 = NA (no ocean) | 3 |  | Selects the dominant small mode aerosol model (largest number of pixels involved in the EDR aggregation) over ocean; See AOT ATBD for all model details |
| Large Mode Aerosol Model (ocean) | 100 = 4 = Coarse mode 5 011 = 3 = Coarse mode 4 010 = 2 = Coarse mode 3 001 = 1 = Coarse mode 2 000 = 0 = Coarse mode 1 111 = 7 = NA (no ocean) | 3 |  | Selects the dominant large mode aerosol model (largest number of pixels involved in the EDR aggregation) over ocean; See AOT ATBD for all model details |

**A.3. Suspended Matter Quality Flags**

**A.3.1. QF1**

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| Flag | Values | Bits | Conditions | Notes |
| Suspended Matter Detection Product Quality | 11 = 3 = High 10 = 2 = Medium 01 = 1 = Low 00 = 0 = Not Produced | 2 | **High:** Pixel SM type quality is good **Medium:** Pixel SM type quality is degraded **Low:** Pixel SM type quality is excluded **Not Produced:** Pixel SM type quality is not produced | Pixel SM type quality is from Aerosol IP product, it is set by default to the Pixel-level AOT quality (see Table 3 for conditions) and then changed under the following conditions: **Excluded:** AOT at 550 nm < 0.5 **Good:** If volcanic ash is detected, SM type quailty is reset to good no matter what the AOT quality is |
| Suspended Matter Type Product Quality | 11 = 3 = High 10 = 2 = Medium 01 = 1 = Low 00 = 0 = Not Produced | 2 | **High:** Pixel SM type quality is good and "Low AOT, SM Typing Excluded" flag is not set (AOT at 550 nm ≤ 0.15 (no SM) or AOT at 550 nm ≥ 0.5) **Medium:** Pixel SM type quality is degraded and "Low AOT, SM Typing Excluded" is not set (AOT at 550 nm ≤ 0.15 (no SM) or AOT at 550 nm ≥ 0.5) **Low:** Pixel SM type quality is good/degraded and "Low AOT, SM Typing Excluded" is set (0.15 < AOT at 550 nm < 0.5) **Not Produced:** Pixel SM type quality is not produced | Pixel SM type quality is from Aerosol IP product, it is set by default to the Pixel-level AOT quality and then changed under the following conditions: **Excluded:** AOT at 550 nm < 0.5 **Good:** If volcanic ash is detected, SM type quailty is reset to good no matter what the AOT quality is Low AOT flag is from Aerosol IP product, it is set under the following conditions: **Yes:** 0.15 < AOT at 550 nm < 0.5 **No:** AOT at 550 nm ≤ 0.15 (no SM), AOT at 550 nm ≥ 0.5 |
| Smoke Concentration Product Quality | 11 = 3 = High 10 = 2 = Medium 01 = 1 = Low 00 = 0 = Not Produced | 2 | **High:** Pixel SM type quality is good and smoke concentration is not larger than the maximum threshold (1000 µg/m3) **Medium:** Pixel SM type quality is degraded and smoke concentration is not larger than the maximum threshold (1000 µg/m3) **Low:** Pixel SM type quality is good/degraded and smoke concentration is larger than the maxiumum threshold (1000 µg/m3) **Not Produced:** Pixel SM type quality is not produced | Pixel SM type quality is from Aerosol IP product |
| Land, Ocean, or Not Produced | 00 = 0 = Land 01 = 1 = Ocean 11 = 3 = Not Produced | 2 | **Land:** Pixel surface type is land or desert **Ocean:** Pixel surface type is sea water | Pixel surface type is from Aerosol IP product |

**A.3.2. QF2**

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| Flag | Values | Bits | Conditions | Notes |
| Cloud Contamination | 1 = Yes 0 = No | 1 | **Yes:** Pixel is not confidently clear |  |
| Cloud adjacent to cell | 1 = Yes 0 = No | 1 | **Yes:** Pixel adjacent cloud flag is confident or probably cloudy |  |
| Cirrus Contamination | 1 = Yes 0 = No | 1 |  | Copied from Aerosol IP Cirrus Quality Flag |
| Bad SDR | 1 = Yes 0 = No | 1 |  | Copied from Aerosol IP Bad SDR Quality Flag |
| Sunglint | 1 = Yes 0 = No | 1 | **Yes:** Pixel has sunglint flag set |  |
| Cloud Shadow | 1 = Yes 0 = No | 1 |  | Copied from Aerosol IP Cloud Shadow Quality Flag |
| Snow/Ice | 1 = Yes 0 = No | 1 |  | Copied from Aerosol IP Snow/Ice Quality Flag |
| Fire | 1 = Yes 0 = No | 1 |  | Copied from Aerosol IP Fire Quality Flag |

**A.3.3. QF3**

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| Flag | Values | Bits | Conditions | Notes |
| Smoke Concentration out of Expected Range | 1 = Yes 0 = No | 1 | **Yes:** Pixel smoke concentration is beyond the expected range (0-1000 µg/m3) |  |
| Excluded SM typing | 1 = Yes 0 = No | 1 |  | Copied from the Aerosol IP SM Typing Excluded Quality Flag |
| Excluded SM Detection | 1 = Yes 0 = No | 1 |  | Copied from the Aerosol IP SM Detection Excluded Quality Flag |
| Low Sun | 1 = Yes 0 = No | 1 | **Yes:** IP day/night flag is set to 'Low sun, degraded' (65º < Solar zenith angle ≤ 80º) | Day/Night flag is from Aerosol IP Product |
| Bright Surface/ Shallow or Turbid Water | 1 = Yes 0 = No | 1 | **Yes:** IP bright pixel or turbid/shallow water flag is set | Bright Surface and Turbid/Shallow Water flag is from Aerosol IP Product |

**Appendix B: Helpful Tools for Working with VIIRS Files**

**B.1 HDF5 Tools**

For users unaccustomed to working with HDF5 formatted files, the HDF Group has a tutorial with example programs and available tools (including HDFView) on their website at <http://www.hdfgroup.org/HDF5/>.

**B.2 IDL Tools**

IDL has a built-in library of commands for HDF5 files. Documentation can be found online at <http://idlastro.gsfc.nasa.gov/idl_html_help/Hierarchical_Data_Format_-_HDF5.html> or using IDL Help.

Also, Michael Galloy has written a particularly helpful IDL program to read HDF5 arrays into IDL. It is available at <http://michaelgalloy.com/lib/hdf5/mg_h5_getdata.html>. Example usages for reading in fields from the VIIRS Aerosol EDR and Aerosol Geolocation is below.

Extracts Latitude and Longitude from Aerosol Geolocation:

Latitude = mg\_h5\_getdata(GAERO\_File, ‘/All\_Data/VIIRS-Aeros-EDR-GEO\_All/Latitude’)

Longitude = mg\_h5\_getdata(GAERO\_File, ‘/All\_Data/VIIRS-Aeros-EDR-GEO\_All/Longitude’)

Extracts Day/Night Metadata from Aerosol Geolocation:

DayNight = mg\_h5\_getdata(GAERO\_File, ‘/Data\_Products/VIIRS-Aeros-EDR-GEO/VIIRS-Aeros-EDR-GEO\_Gran\_0.N\_Day\_Night\_Flag’)

Extracts AOT and AOT Scale and Offset from Aerosol EDR and converts to floating point numbers:

AOT = mg\_h5\_getdata(VAOOO\_File, ‘/All\_Data/VIIRS-Aeros-EDR\_All/AerosolOpticalDepth\_at\_550nm’)

AOT\_Factors = mg\_h5\_getdata(VAOOO\_File, ‘/All\_Data/VIIRS-Aeros-EDR\_All/AerosolOpticalDepthFactors’)

AOT\_float = (AOT \* AOT\_Factors[0]) + AOT\_Factors[1]